Name: Mayank


Course: B.Sc. (H) Computer Science

Roll No.: 20221468


Practical :Computer network

Q1. To Study basic network command and Network configuration commands.


1.ping




2.ipconfig




3. tracert



4. nslookup



5. netstat



Q2. To study and perform PC to PC communication.

Steps to be followed:

1: Open Cisco Packet tracer Application

2: Create new file and add 2 PCs to the screen by dragging from bottom of screen


3: Connect the 2 PCs using cables and use any cable u like. In my case I am using crossover cable and adding fast ethernet to both.

4: To assign ip to PC click on PC🡪Desktop🡪IP Configuration and type ip address 192.168.1.1 on 1st PC and 192.168.1.2 on 2nd PC.

5: Then select add sample PDU and select the origin PC and destination PC.

6: Use simulation and see how packet is travelling.

Output:




Q3. To create Star topology using Hub and Switch.

Steps:

1. Add PCs and a switch in between on one part of screen and more PCs and hub on the other part of the screen.
2. Connect each device to hub and switch
3. Configure each ip address for all devices as shown in picture like 172.16.0.1 etc.
4. To check connection ping a PC 172.16.0.1 with 172.16.0.4, use command ping 172.16.0.4 on pc1.
5. Select add sample PDU and select origin and destination PC using simulation see how packet is transferring.

Output:



Q4. To create Bus, Ring, Tree, Hybrid, Mesh topologies.

1. Add PCs and corresponding switches according to the topologies



2. Connect each device to switch according to topologies

3. Configure IP addresses for all PCs

4. Check connection using ping command

5. Add sample PDU and see simulation

Output:




Q5. Perform an initial Switch configuration.

Steps:

1. Open Cisco Packet tracer
2. Drag and drop switch from bottom left area to workspace
3. Connect a PC if u want to the switch using ethernet cables
4. Access switch CLI and enter enable command
5. Examine the current switch configuration by show running-config command.
6. Enter command configure terminal🡪hostname test
7. Verify Configuration by running: show interfaces, show vlan, show ip interface brief.

Output:




Q6. Perform an initial Router configuration.

Steps:

1. Open Cisco Packet Tracer
2. Drag and drop Router
3. Connect devices
4. Access router CLI
5. Configure router using following commands: enable🡪 configure terminal🡪 hostname mayank
6. Configure interfaces use command: interface🡪ip address🡪no shutdown
7. Configure default gateway: ip default-gateway 192.168.0.1
8. Verify Configuration: show interfaces🡪show ip interface brief🡪show ip route
9. Exit: exit

Output:



Q7. To implement Client-server Network.

Steps:

1. Launch Cisco Packet Tracer and create a new empty workspace.

2. Drag and drop devices from the “End Devices” and "Routers" sections to design your network topology.


3.Connect the devices using appropriate cables (Ethernet, Serial, etc.) to establish network connectivity and add ip addresses to each.


4. Add and configure the server, make changes in server http and dns

5. Configure Client

6. Test Connectivity using ping command

Output:





Q8. To implement connection between devices using router.

Steps:

1. Design the topology using devices and cables
2. Configure Ip addresses on the devices add ip addresses on both laptops
3. Configure routing go to router 🡪config then in Gigabit Ethernet 0/0/0 turn it on and put ip address and in gigabit Ethernet 0/0/1 turn it on and put ip
4. Test Connectivity using simulation

Output:

